* Why is your 100uF cap labeled as 1uF?
* Vcc plane is heavily constricted, especially around your IMU and radio
* Your ground plane is also heavily constricted
* Your oscillator is too far away from your MCU, and the traces are not well laid out. Follow this guideline: [link](https://electronics.stackexchange.com/questions/39136/competing-pcb-crystal-layout-recommendations)